SPACE TELESCOPE SCIENCE INSTITUTE

Summary: 16 September - 22 October 1996

Instrument: Nominal operation (1 new dead diode identified) Acquisition: 55 total; 3 failures; 1 GS LOL; one 8-steps to success Science: 38 GO/GTO programs; 4 visits lost Calibration: 6 programs (Darks, YBASEs, Wavecals, Polarimetry, Photometry) Other:

IS Reviews: 11 completed.

Paper Product Reviews: 25 completed, 9 pending.

SPACE TELESCOPE SCIENCE INSTITUTE

Instrument Status (16 September - 22 October 1996):

FOS instrumental operation nominal

- 1 dead diode identified (FOS/RD 154, affects pixels 612-632)

- commanding and dead diode table (DDT) updates in process

- FOS/RD G400H flat field change - new flat to be delivered

- fastest RAPID ever (60 minutes of 0.035 sec readouts) succeeded

- PERIOD mode observations obtained

- pointing near Moon successful

Target Acquisition Problems:

- two crowded field failures(6831 and 6696)

- algorithm aborts rather than return to brightest

- all subsequent science exposures off targets

- one target too faint (6589); GO coord error

- one guide star loss-of-lock (GS LOL) (6799); all exposures lost

- one 8-steps to success (6823); all OK

- algorithm iteration limit exceeded - required correction ~0.02 arcsec

TIPS: 24 October 1996 FOS Keyes